(module MikroBus-SMD (layer F.Cu) (tedit 5E442486)
  (attr smd)
  (fp_text reference REF** (at 0 -1.27) (layer F.SilkS))
  (fp_text value MikroBus-SMD (at 0 0) (layer F.Fab))
  (fp_text user %R (at 11.43 0 90) (layer F.Fab))
  (fp_text user %R (at -11.43 0 90) (layer F.Fab))
  (pad 10 smd rect (at 13.08 6.35) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 13.08 1.27) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 13.08 -3.81) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 13.08 -8.89) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 9.78 8.89) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 9.78 3.81) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 9.78 -1.27) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 9.78 -6.35) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -13.08 8.89) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -13.08 3.81) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -13.08 -6.35) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -9.78 -8.89) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -13.08 -1.27) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -9.78 6.35) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -9.78 -3.81) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -9.78 1.27) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
    (offset (xyz 11.43 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
    (offset (xyz -11.43 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
